# Index

A B C D E F G H I J L M N O P R S T U V W
All Classes|All Packages

## I

IDataRequest<DataType> - Interface in com.mouseviator.fsuipc.datarequest
  This interface is used by many functions in `FSUIPC` class.
IDataRequest.RequestType - Enum in com.mouseviator.fsuipc.datarequest
  This enumeration defines the possible types of data request.
identityOffset - Variable in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper
IFSUIPCListener - Interface in com.mouseviator.fsuipc
  This interface to be implemented to receive notifications from `FSUIPC` library.
ilsGlideSlopeInclinationOffset - Variable in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper
ilsInverseRunwayHeadingOffset - Variable in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper
INFO - com.mouseviator.fsuipc.FSUIPCWrapper.LogSeverity
IntegerLVarReadRequest(int) - Constructor for class com.mouseviator.fsuipc.helpers.LVarHelper.IntegerLVarReadRequest
  Construct new LVar read request.
IntegerLVarWriteRequest(int, Integer) - Constructor for class com.mouseviator.fsuipc.helpers.LVarHelper.IntegerLVarWriteRequest
  Construct new LVar write request.
IntRequest - Class in com.mouseviator.fsuipc.datarequest.primitives
  This class implements integer data request for use with `FSUIPC` class.
IntRequest() - Constructor for class com.mouseviator.fsuipc.datarequest.primitives.IntRequest
  Creates a new integer data request.
IntRequest(int) - Constructor for class com.mouseviator.fsuipc.datarequest.primitives.IntRequest
  Creates a new integer data request associated with given offset.
IntRequest(int, int) - Constructor for class com.mouseviator.fsuipc.datarequest.primitives.IntRequest
  Creates a new integer data request associated with given offset and with given value.This also sets data request type to WRITE.
IntRequest(int, Integer) - Constructor for class com.mouseviator.fsuipc.datarequest.primitives.IntRequest
  Creates a new integer data request associated with given offset and with given value.This also sets data request type to WRITE.
IReadOnlyRequest<DataType> - Interface in com.mouseviator.fsuipc.datarequest
  This interface extends the `IDataRequest` interface and should be used when implementing data request, that is read only, as it provides default implementation of `IDataRequest.setValue(java.lang.Object)` function, which causes exception every once called.
isAvailable() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.BackCourseFlags
  Tests whether bit 0 - BC available, is set or not.
isConnected() - Method in class com.mouseviator.fsuipc.FSUIPC
  Will return the value of the internal `AtomicBoolean` variable that is being updated when FSUIPC is connected/disconnected.
isDMEActive() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.CodeFlags
  Tests whether bit 0 - DME available, is set or not.
isDMEGSColocated() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.CodeFlags
  Tests whether bit 4 - DME/GS co-located (Not found for FSX), is set or not.
isGSAvailable() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.CodeFlags
  Tests whether bit 6 - GS available, is set or not.
isLocaliserTunedIn() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.BackCourseFlags
  Tests whether bit 1 - Localiser tuned in, is set or not.
isNoBackCourse() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.CodeFlags
  Tests whether bit 5 - No back course, is set or not.
isNoSignal() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.CodeFlags
  Tests whether bit 3 - No signal available, is set or not.
isOnBackCourse() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.BackCourseFlags
  Tests whether bit 4 - On Back Course (Not found for FSX), is set or not.
isStationActive() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.BackCourseFlags
  Tests whether bit 7 - Station active (even if no BC), is set or not.
isStationActive() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.CodeFlags
  Tests whether bit 7 - This is a localiser (else it’s a VOR), is set or not.
isTACAN() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.CodeFlags
  Tests whether bit 1 - TACAN (Not found for FSX), is set or not.
isVoiceAvailable() - Method in class com.mouseviator.fsuipc.helpers.avionics.NavRadioHelper.CodeFlags
  Tests whether bit 2 - Voice available (Not found for FSX), is set or not.
IWriteOnlyRequest<DataType> - Interface in com.mouseviator.fsuipc.datarequest
  This interface extends the `IDataRequest` interface and should be used when implementing data request, that is write only, as it provides default implementation of `IDataRequest.getValue()` function, which causes exception every once called.

A B C D E F G H I J L M N O P R S T U V W
All Classes|All Packages